**Module Design Document**

**For**

**VrfyCritReg**

**Apr 14, 2016**

**Prepared For:**

**Software Engineering**

**Nexteer Automotive,**

**Saginaw, MI, USA**

**Prepared By:**

**Selva Sengottaiyan**

**Nexteer Automotive,**

**Saginaw, MI, USAChange History**

|  |  |  |  |
| --- | --- | --- | --- |
| **Description** | **Author** | **Version** | **Date** |
| Initial Version | Sankardu Varadapureddi | 1 | 14-Jan-2016 |
| Updated to “ Critical register” checks at init and periodic functions | Selva Sengottaiyan | 2 | 14-Apr-2016 |

**Table of Contents**

[1 Introduction 5](#_Toc440635612)

[1.1 Purpose 5](#_Toc440635613)

[1.2 Scope 5](#_Toc440635614)

[2 VrfyCritReg High-Level Description 6](#_Toc440635615)

[3 Design details of software module 7](#_Toc440635616)

[3.1 Graphical representation of VrfyCritReg 7](#_Toc440635617)

[3.2 Data Flow Diagram 7](#_Toc440635618)

[3.2.1 Component level DFD 7](#_Toc440635619)

[3.2.2 Function level DFD 7](#_Toc440635620)

[4 Constant Data Dictionary 8](#_Toc440635621)

[4.1 Program (fixed) Constants 8](#_Toc440635622)

[4.1.1 Embedded Constants 8](#_Toc440635623)

[5 Software Component Implementation 9](#_Toc440635624)

[5.1 Sub-Module Functions 9](#_Toc440635625)

[5.1.1 Init: VrfyCritRegInit1 9](#_Toc440635626)

[5.1.1.1 Design Rationale 9](#_Toc440635627)

[5.1.1.2 Module Outputs 9](#_Toc440635628)

[5.1.2 Per: VrfyCritRegPer1 9](#_Toc440635629)

[5.1.2.1 Design Rationale 9](#_Toc440635630)

[5.1.2.2 Store Module Inputs to Local copies 9](#_Toc440635631)

[5.1.2.3 (Processing of function)……… 9](#_Toc440635632)

[5.1.2.4 Store Local copy of outputs into Module Outputs 9](#_Toc440635633)

[5.2 Server Runables 9](#_Toc440635634)

[5.3 Interrupt Functions 9](#_Toc440635635)

[5.4 Module Internal (Local) Functions 9](#_Toc440635636)

[5.4.1 Local Function #2 9](#_Toc440635637)

[5.4.1.1 Description 9](#_Toc440635638)

[5.5 GLOBAL Function/Macro Definitions 10](#_Toc440635639)

[6 Known Limitations with Design 11](#_Toc440635640)

[7 UNIT TEST CONSIDERATION 12](#_Toc440635641)

[Appendix A Abbreviations and Acronyms 13](#_Toc440635642)

[Appendix B Glossary 14](#_Toc440635643)

[Appendix C References 15](#_Toc440635644)

# Introduction

## Purpose


## Scope

# VrfyCritReg High-Level Description

Refer to FDD

# Design details of software module

## Graphical representation of VrfyCritReg



## Data Flow Diagram

Refer FDD

### Component level DFD

### Function level DFD

# Constant Data Dictionary

## Program (fixed) Constants

### Embedded Constants

Refer .m file

#### Local Constants

|  |  |  |
| --- | --- | --- |
| Constant Name | Data Type | Value |
| SYSCRITREGFLT\_CNT\_U08 | uint8 | 2 |
| CRITREGFLT\_CNT\_U08 | uint8 | 1 |
| NOFLT\_CNT\_U08 | uint8 | 0 |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# Software Component Implementation

## Sub-Module Functions

## Init: VrfyCritRegInit1

## Design Rationale

*Refer FDD*

## Module Outputs

*None*

## Per: VrfyCritRegPer1

## Design Rationale

Refer FDD

## Store Module Inputs to Local copies

*None*

## (Processing of function)………

*Refer FDD*

## Store Local copy of outputs into Module Outputs

*None*

## Server Runables

*None*

## Interrupt Functions

*None*

## Module Internal (Local) Functions

## Local Function #1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Function Name** | SysCritReg<Register Short Name>IninChk | Type | Min | | Max |
| **Arguments Passed** | NA |  |  |  | |
| **Return Value** | &SysRegsOk\_Uls\_T\_lgc | boolean | FALSE | TRUE | |

## Description

Set ' SysRegsOk\_Uls\_T\_lgc to FALSE if CPU System Register values are not equal to expected values. This is configured to be called from trusted function because it needs to run in supervisor mode

## Local Function #2

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Function Name** | SysCritReg<Register Short Name>PerChk | Type | Min | | Max |
| **Arguments Passed** | NA |  |  |  | |
| **Return Value** | &SysRegsOk\_Uls\_T\_lgc | boolean | FALSE | TRUE | |

## Description

Set ' SysRegsOk\_Uls\_T\_lgc to FALSE if CPU System Register values are not equal to expected values. This is configured to be called from trusted function because it needs to run in supervisor mode

## 

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  |  |  | |  |
|  |  |  |  |  | |
|  |  |  |  |  | |

## 

## GLOBAL Function/Macro Definitions

## Global1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | CritRegPerChk |  |  | |  |
|  |  |  |  |  | |
|  | NtcParamInfo\_Cnt\_T\_u08 | uint8 | 0U | 2U | |

NtcParamInfo\_Cnt\_T\_u081Non Set ' NtcParamInfo\_Cnt\_T\_u08 to 2 if CPU System Register values are not equal to expected values. Set ' NtcParamInfo\_Cnt\_T\_u08 to 0 if none of the above conditions are true.

## Global Function #2

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Function Name** | CritRegInitChk | Type | Min | | Max |
| **Arguments Passed** | NA |  |  |  | |
| **Return Value** | NtcParamInfo\_Cnt\_T\_u08 | uint8 | 0U | 2U | |

## Description

Set ' NtcParamInfo\_Cnt\_T\_u08 to 1 if CPU Non System Register values are not equal to expected values. Set ' NtcParamInfo\_Cnt\_T\_u08 to 2 if CPU System Register values are not equal to expected values. Set ' NtcParamInfo\_Cnt\_T\_u08 to 0 if none of the above conditions are true. This is configured as a trusted function because it needs to run in supervisor mode

## Global Function #3

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Function Name** | SysCritRegIninChk | Type | Min | | Max |
| **Arguments Passed** | NA |  |  |  | |
| **Return Value** | SysRegsOk\_Uls\_T\_lgc | boolean | FALSE | TRUE | |

## Description

Set ' SysRegsOk\_Uls\_T\_lgc to FALSE if CPU System Register values are not equal to expected values. This is configured to be called from trusted function because it needs to run in supervisor mode

## Global Function #4

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Function Name** | SysCritRegPerChk | Type | Min | | Max |
| **Arguments Passed** | NA |  |  |  | |
| **Return Value** | SysRegsOk\_Uls\_T\_lgc | boolean | FALSE | TRUE | |

## Description

Set ' SysRegsOk\_Uls\_T\_lgc to FALSE if CPU System Register values are not equal to expected values. This is configured to be called from trusted function because it needs to run in supervisor mode

# Known Limitations with Design

# UNIT TEST CONSIDERATION

None

Abbreviations and Acronyms

| **Abbreviation or Acronym** | **Description** |
| --- | --- |
|  |  |
|  |  |

Glossary

**Note**: Terms and definitions from the source “Nexteer Automotive” take precedence over all other definitions of the same term. Terms and definitions from the source “Nexteer Automotive” are formulated from multiple sources, including the following:

* ISO 9000
* ISO/IEC 12207
* ISO/IEC 15504
* Automotive SPICE® Process Reference Model (PRM)
* Automotive SPICE® Process Assessment Model (PAM)
* ISO/IEC 15288
* ISO 26262
* IEEE Standards
* SWEBOK
* PMBOK
* Existing Nexteer Automotive documentation

| **Term** | **Definition** | **Source** |
| --- | --- | --- |
| MDD | Module Design Document |  |
| DFD | Data Flow Diagram |  |

References

| **Ref. #** | **Title** | **Version** |
| --- | --- | --- |
| 1 | AUTOSAR Specification of Memory Mapping (Link:[AUTOSAR\_SWS\_MemoryMapping.pdf](http://www.autosar.org/download/R4.0/AUTOSAR_SWS_MemoryMapping.pdf)) | v1.3.0 R4.0 Rev 2 |
| 2 | MDD Guideline | EA4 01.00.01 |
| 3 | [Software Naming Conventions.doc](http://misagweb01.nexteer.com/eRoomReq/Files/erooms8/NextGeneration/0_fc55f/Software%20Naming%20Conventions%2003x(In%20Work).doc) | EA4 01.00.01 |
| 4 | [Software Design and Coding Standards.doc](http://eroom1.nexteer.com/eRoomReq/Files/erooms8/NextGeneration/0_1a67a9/Software%20Design%20and%20Coding%20Standards.doc) | 2.1 |
| 5 | FDD : CM111A\_VrfyCritReg\_Design | See Synergy sub project version |