**Module Design Document**

**For**

**ExcpnHndlg**

**April 5, 2016**

**Prepared For:**

**Software Engineering**

**Nexteer Automotive,**

**Saginaw, MI, USA**

**Prepared By:**

**Software Group,**

**Nexteer Automotive,**

**Saginaw, MI, USAChange History**

|  |  |  |  |
| --- | --- | --- | --- |
| **Description** | **Author** | **Version** | **Date** |
| Initial Version | Avinash James | 1.0 | 05-Apr-2016 |

**Table of Contents**

[1 Introduction 7](#_Toc447790852)

[1.1 Purpose 7](#_Toc447790853)

[1.2 Scope 7](#_Toc447790854)

[2 ExcpnHndlg & High-Level Description 8](#_Toc447790855)

[3 Design details of software module 9](#_Toc447790856)

[3.1 Graphical representation of ExcpnHndlg 9](#_Toc447790857)

[3.2 Data Flow Diagram 9](#_Toc447790858)

[3.2.1 Component level DFD 9](#_Toc447790859)

[3.2.2 Function level DFD 9](#_Toc447790860)

[4 Constant Data Dictionary 10](#_Toc447790861)

[4.1 Program (fixed) Constants 10](#_Toc447790862)

[4.1.1 Embedded Constants 10](#_Toc447790863)

[5 Software Component Implementation 13](#_Toc447790864)

[5.1 Sub-Module Functions 13](#_Toc447790865)

[5.1.1 Init: ExcpnHndlgInit1 13](#_Toc447790866)

[5.1.1.1 Design Rationale 13](#_Toc447790867)

[5.1.1.2 Module Outputs 13](#_Toc447790868)

[5.1.2 Init: ExcpnHndlgInit2 13](#_Toc447790869)

[5.1.2.1 Design Rationale 13](#_Toc447790870)

[5.1.2.2 Module Outputs 13](#_Toc447790871)

[5.1.3 Per: ExcpnHndlgPer1 13](#_Toc447790872)

[5.1.3.1 Design Rationale 13](#_Toc447790873)

[5.1.3.2 Store Module Inputs to Local copies 13](#_Toc447790874)

[5.1.3.3 (Processing of function)……… 13](#_Toc447790875)

[5.1.3.4 Store Local copy of outputs into Module Outputs 13](#_Toc447790876)

[5.2 Server Runables 13](#_Toc447790877)

[5.2.1 ChkForStrtUpTest 13](#_Toc447790878)

[5.2.1.1 Design Rationale 13](#_Toc447790879)

[5.2.1.2 (Processing of function)……… 13](#_Toc447790880)

[5.2.2 FeNmiClkMonr0RtLowrLimFlt 14](#_Toc447790881)

[5.2.2.1 Design Rationale 14](#_Toc447790882)

[5.2.2.2 (Processing of function)……… 14](#_Toc447790883)

[5.2.3 FeNmiClkMonr0RtUpprLimFlt 14](#_Toc447790884)

[5.2.3.1 Design Rationale 14](#_Toc447790885)

[5.2.3.2 (Processing of function)……… 14](#_Toc447790886)

[5.2.4 FeNmiClkMonr1RtLowrLimFlt 14](#_Toc447790887)

[5.2.4.1 Design Rationale 14](#_Toc447790888)

[5.2.4.2 (Processing of function)……… 14](#_Toc447790889)

[5.2.5 FeNmiClkMonr1RtUpprLimFlt 14](#_Toc447790890)

[5.2.5.1 Design Rationale 14](#_Toc447790891)

[5.2.5.2 (Processing of function)……… 14](#_Toc447790892)

[5.2.6 FeNmiClkMonr2RtLowrLimFlt 14](#_Toc447790893)

[5.2.6.1 Design Rationale 14](#_Toc447790894)

[5.2.6.2 (Processing of function)……… 14](#_Toc447790895)

[5.2.7 FeNmiClkMonr2RtUpprLimFlt 14](#_Toc447790896)

[5.2.7.1 Design Rationale 14](#_Toc447790897)

[5.2.7.2 (Processing of function)……… 15](#_Toc447790898)

[5.2.8 FeNmiClkMonr3RtLowrLimFlt 15](#_Toc447790899)

[5.2.8.1 Design Rationale 15](#_Toc447790900)

[5.2.8.2 (Processing of function)……… 15](#_Toc447790901)

[5.2.9 FeNmiClkMonr3RtUpprLimFlt 15](#_Toc447790902)

[5.2.9.1 Design Rationale 15](#_Toc447790903)

[5.2.9.2 (Processing of function)……… 15](#_Toc447790904)

[5.2.10 FeNmiDmaTrf 15](#_Toc447790905)

[5.2.10.1 Design Rationale 15](#_Toc447790906)

[5.2.10.2 (Processing of function)……… 15](#_Toc447790907)

[5.2.11 FeNmiDmaRegAcsProtnErr 15](#_Toc447790908)

[5.2.11.1 Design Rationale 15](#_Toc447790909)

[5.2.11.2 (Processing of function)……… 15](#_Toc447790910)

[5.2.12 FeNmiEcmMstChkrCmp 15](#_Toc447790911)

[5.2.12.1 Design Rationale 15](#_Toc447790912)

[5.2.12.2 (Processing of function)……… 15](#_Toc447790913)

[5.2.13 FeNmiOperModErrFlsProgmModStrtd 16](#_Toc447790914)

[5.2.13.1 Design Rationale 16](#_Toc447790915)

[5.2.13.2 (Processing of function)……… 16](#_Toc447790916)

[5.2.14 FeNmiOperModErrSngChipInactv 16](#_Toc447790917)

[5.2.14.1 Design Rationale 16](#_Toc447790918)

[5.2.14.2 (Processing of function)……… 16](#_Toc447790919)

[5.2.15 FeNmiOperModErrTestModStrtd 16](#_Toc447790920)

[5.2.15.1 Design Rationale 16](#_Toc447790921)

[5.2.15.2 (Processing of function)……… 16](#_Toc447790922)

[5.2.16 FeNmiPeg 16](#_Toc447790923)

[5.2.16.1 Design Rationale 16](#_Toc447790924)

[5.2.16.2 (Processing of function)……… 16](#_Toc447790925)

[5.2.17 FeNmiWdg 16](#_Toc447790926)

[5.2.17.1 Design Rationale 16](#_Toc447790927)

[5.2.17.2 (Processing of function)……… 16](#_Toc447790928)

[5.2.18 GetMcuDiagcIdnData 17](#_Toc447790929)

[5.2.18.1 Design Rationale 17](#_Toc447790930)

[5.2.18.2 (Processing of function)……… 17](#_Toc447790931)

[5.2.19 ProcMpuExcpnErr 17](#_Toc447790932)

[5.2.19.1 Design Rationale 17](#_Toc447790933)

[5.2.19.2 (Processing of function)……… 17](#_Toc447790934)

[5.2.20 ProcNonCritOsErr 17](#_Toc447790935)

[5.2.20.1 Design Rationale 17](#_Toc447790936)

[5.2.20.2 (Processing of function)……… 17](#_Toc447790937)

[5.2.21 ProcPrmntOsErr 17](#_Toc447790938)

[5.2.21.1 Design Rationale 17](#_Toc447790939)

[5.2.21.2 (Processing of function)……… 17](#_Toc447790940)

[5.2.22 ProcPrvlgdInstrExcpnErr 17](#_Toc447790941)

[5.2.22.1 Design Rationale 17](#_Toc447790942)

[5.2.22.2 (Processing of function)……… 17](#_Toc447790943)

[5.2.23 ProcUkwnExcpnErr 18](#_Toc447790944)

[5.2.23.1 Design Rationale 18](#_Toc447790945)

[5.2.23.2 (Processing of function)……… 18](#_Toc447790946)

[5.2.24 SetMcuDiagcIdnData 18](#_Toc447790947)

[5.2.24.1 Design Rationale 18](#_Toc447790948)

[5.2.24.2 (Processing of function)……… 18](#_Toc447790949)

[5.3 Interrupt Functions 18](#_Toc447790950)

[5.3.1 AlgnErrIrq 18](#_Toc447790951)

[5.3.1.1 Design Rationale 18](#_Toc447790952)

[5.3.1.2 (Processing of the ISR function)….. 18](#_Toc447790953)

[5.3.2 FpuErrIrq 18](#_Toc447790954)

[5.3.2.1 Design Rationale 18](#_Toc447790955)

[5.3.2.2 (Processing of the ISR function)….. 18](#_Toc447790956)

[5.3.3 SysErrIrq 18](#_Toc447790957)

[5.3.3.1 Design Rationale 18](#_Toc447790958)

[5.3.3.2 (Processing of the ISR function)….. 18](#_Toc447790959)

[5.3.4 ResdOperIrq 19](#_Toc447790960)

[5.3.4.1 Design Rationale 19](#_Toc447790961)

[5.3.4.2 (Processing of the ISR function)….. 19](#_Toc447790962)

[5.4 Module Internal (Local) Functions 19](#_Toc447790963)

[5.4.1 ProcStrtUpOrSwRst 19](#_Toc447790964)

[5.4.1.1 Design Rationale 19](#_Toc447790965)

[5.4.1.2 Processing 19](#_Toc447790966)

[5.4.2 ProcEcmRst 19](#_Toc447790967)

[5.4.2.1 Design Rationale 19](#_Toc447790968)

[5.4.2.2 Processing 19](#_Toc447790969)

[5.4.3 ProcPinRst 19](#_Toc447790970)

[5.4.3.1 Design Rationale 20](#_Toc447790971)

[5.4.3.2 Processing 20](#_Toc447790972)

[5.5 GLOBAL Function/Macro Definitions 20](#_Toc447790973)

[5.5.1 GLOBAL Function #1 20](#_Toc447790974)

[5.5.1.1 Design Rationale 20](#_Toc447790975)

[5.5.1.2 processing 20](#_Toc447790976)

[6 Known Limitations with Design 21](#_Toc447790977)

[7 UNIT TEST CONSIDERATION 22](#_Toc447790978)

[Appendix A Abbreviations and Acronyms 23](#_Toc447790979)

[Appendix B Glossary 24](#_Toc447790980)

[Appendix C References 25](#_Toc447790981)

# Introduction

## Purpose

This document details the design in the FDD and also lists out any deviations which were made from the design for the implementation due to any constraints in development. ExcpnHndlg MDD describes the exception handling / reset cause determination for microcontroller diagnostics

## Scope

The following definitions are used throughout this document:

* **Shall**: indicates a mandatory requirement without exception in compliance.
* **Should**: indicates a mandatory requirement; exceptions allowed only with documented justification.
* **May**: indicates an optional action.


# ExcpnHndlg & High-Level Description

Refer FDD

# Design details of software module

## Graphical representation of ExcpnHndlg

## Data Flow Diagram



### Component level DFD

**N/A**

### Function level DFD

**N/A**

# Constant Data Dictionary

## Program (fixed) Constants

### Embedded Constants

#### Local Constants

|  |  |  |  |
| --- | --- | --- | --- |
| Constant Name | Resolution | Units | Value |
| FPCFGININVAL\_CNT\_T\_U32 | 1 | Counts | 0x0000001CU |
| FPCFGREGID\_CNT\_S32 | 1 | Counts | 10 |
| FPCFGSELNID\_CNT\_S32 | 1 | Counts | 0 |
| FPUINVLDOPERSTSBIT\_CNT\_U32 | 1 | Counts | ((uint32)(0x00004000U)) |
| FPUDIVBYZEROSTSBIT\_CNT\_U32 | 1 | Counts | ((uint32)(0x00002000U)) |
| FPUOVFSTSBIT\_CNT\_U32 | 1 | Counts | ((uint32)(0x00001000U)) |
| MEMERRINFOREADWRBIT\_CNT\_U32 | 1 | Counts | ((uint32)(0x00000001U)) |
| CF1STERSTRADRPARMASK\_CNT\_U32 | 1 | Counts | ((uint32)(0x00000004U)) |
| CF1STERSTRDBLBITMASK\_CNT\_U32 | 1 | Counts | ((uint32)(0x00000002U)) |
| CF1STERSTRSNGBITMASK\_CNT\_U32 | 1 | Counts | ((uint32)(0x00000001U)) |
| PRPHLBUSDATAPARMASK\_CNT\_U32 | 1 | Counts | ((uint32)(0x10000000U)) |
| DTSDBLBITMASK\_CNT\_U32 | 1 | Counts | ((uint32)(0x80000000U)) |
| CODFLSSNGBITHARDFLT\_CNT\_U08 | 1 | Counts | 1U |
| CODFLSECCDBLBIT\_CNT\_U08 | 1 | Counts | 2U |
| CODFLSADRPAR\_CNT\_U08 | 1 | Counts | 4U |
| MEMBISTSTRTUPTESTFAILR\_CNT\_U08 | 1 | Counts | 1U |
| LCLRAMECCSNGBITHARDFLT\_CNT\_U08 | 1 | Counts | 1U |
| LCLRAMECCDBLBIT\_CNT\_U08 | 1 | Counts | 2U |
| INVLDRAMAREA\_CNT\_U08 | 1 | Counts | 4U |
| DTSDBLBIT\_CNT\_U08 | 1 | Counts | 2U |
| SPI0PRPHLRAMDBLBIT\_CNT\_U08 | 1 | Counts | 2U |
| SPI1PRPHLRAMDBLBIT\_CNT\_U08 | 1 | Counts | 2U |
| SPI2PRPHLRAMDBLBIT\_CNT\_U08 | 1 | Counts | 2U |
| SPI3PRPHLRAMDBLBIT\_CNT\_U08 | 1 | Counts | 2U |
| BISTCODECCFAILR\_CNT\_U08 | 1 | Counts | 1U |
| LOGLBISTSTRTUPTESTFAILR\_CNT\_U08 | 1 | Counts | 4U |
| BISTNOTCMPL\_CNT\_U08 | 1 | Counts | 16U |
| CPULOCKSTEPSTRTUPTESTFAILR\_CNT\_U08 | 1 | Counts | 32U |
| LOCKSTEPCOMP\_CNT\_U08 | 1 | Counts | 1U |
| SYSVCIE\_CNT\_U08 | 1 | Counts | 2U |
| RESDOPER\_CNT\_U08 | 1 | Counts | 4U |
| ALGNREAD\_CNT\_U08 | 1 | Counts | 8U |
| ALGNWR\_CNT\_U08 | 1 | Counts | 16U |
| INSTRFETCH\_CNT\_U08 | 1 | Counts | 32U |
| CLKMONR0RTLOWRLIMFLT\_CNT\_U08 | 1 | Counts | 4U |
| CLKMONR0RTUPPRLIMFLT\_CNT\_U08 | 1 | Counts | 8U |
| CLKMONR2RTLOWRLIMFLT\_CNT\_U08 | 1 | Counts | 64U |
| CLKMONR2RTUPPRLIMFLT\_CNT\_U08 | 1 | Counts | 128U |
| OPERMODERRFLSPROGMMODSTRTD\_CNT\_U08 | 1 | Counts | 1U |
| OPERMODERRTESTMODSTRTD\_CNT\_U08 | 1 | Counts | 2U |
| OPERMODERRSNGCHIPINACTV\_CNT\_U08 | 1 | Counts | 4U |
| CLKMONR1RTLOWRLIMFLT\_CNT\_U08 | 1 | Counts | 4U |
| CLKMONR1RTUPPRLIMFLT\_CNT\_U08 | 1 | Counts | 8U |
| CLKMONR3RTLOWRLIMFLT\_CNT\_U08 | 1 | Counts | 64U |
| CLKMONR3RTUPPRLIMFLT\_CNT\_U08 | 1 | Counts | 128U |
| DATAPROTNERR\_CNT\_U08 | 1 | Counts | 1U |
| INSTRPROTNERR\_CNT\_U08 | 1 | Counts | 2U |
| ECMSTSFLT\_CNT\_U08 | 1 | Counts | 1U |
| ECMMSTSTRTUPTESTFAILR\_CNT\_U08 | 1 | Counts | 4U |
| ECMCHKRSTRTUPTESTFAILR\_CNT\_U08 | 1 | Counts | 8U |
| ECMRTMSTCHKRCOMPFLT\_CNT\_U08 | 1 | Counts | 128U |
| FPUINVLDOPEREXCPN\_CNT\_U08 | 1 | Counts | 2U |
| FPUDIVBYZEROEXCPN\_CNT\_U08 | 1 | Counts | 4U |
| FPUOVFEXCPN\_CNT\_U08 | 1 | Counts | 8U |
| FPUUKWNEXCPN\_CNT\_U08 | 1 | Counts | 16U |
| UKWNRST\_CNT\_U08 | 1 | Counts | 1U |
| UKWNECMRST\_CNT\_U08 | 1 | Counts | 2U |
| UKWNSWRST\_CNT\_U08 | 1 | Counts | 16U |
| BACKUPRAMTSTFAILR\_CNT\_U08 | 1 | Counts | 32U |
| FLSBTLDRPREOSSRTUPEXCPN\_CNT\_U08 | 1 | Counts | 64U |
| STRTUPRSTINFOFAILD\_CNT\_U08 | 1 | Counts | 128U |
| PROGFLOW\_CNT\_U08 | 1 | Counts | 1U |
| DEADLINEMONR\_CNT\_U08 | 1 | Counts | 2U |
| ALVMONR\_CNT\_U08 | 1 | Counts | 4U |
| WDGTOUT\_CNT\_U08 | 1 | Counts | 1U |
| PEGRTFLT\_CNT\_U08 | 1 | Counts | 2U |
| IPGRTFLT\_CNT\_U08 | 1 | Counts | 8U |
| PBGSTRTUPTSTAILR\_CNT\_U08 | 1 | Counts | 16U |
| PBGRTFLT\_CNT\_U08 | 1 | Counts | 32U |
| DBGRST\_CNT\_U08 | 1 | Counts | 1U |
| OSCRITFLT\_CNT\_U08 | 1 | Counts | 1U |
| UKWNEXCPN\_CNT\_U08 | 1 | Counts | 2U |
| OSNONCRITFLT\_CNT\_U08 | 1 | Counts | 1U |
| DMATRFERR\_CNT\_U08 | 1 | Counts | 1U |
| DMAREGACSPROTCNERR\_CNT\_U08 | 1 | Counts | 2U |
| PRPHLBUSDATAPARSTRTUPFLT\_CNT\_U08 | 1 | Counts | 64U |
| PRPHLBUSDATAPARPRTFLT\_CNT\_U08 | 1 | Counts | 128U |
| CVMOVERVLTGSTRTUPTESTFAILR\_CNT\_U08 | 1 | Counts | 1U |
| CVMUNDERVLTGSTRTUPTESTFAILR\_CNT\_U08 | 1 | Counts | 2U |
| INTCVMOVERVLTGMONR\_CNT\_U08 | 1 | Counts | 1U |
| INTCVMUNDERVLTGMONR\_CNT\_U08 | 1 | Counts | 2U |
| INTMONRLOVCCFLT\_CNT\_U08 | 1 | Counts | 16U |
| EXTVLTGMONRFLT\_CNT\_U08 | 1 | Counts | 128U |
| UPPR16BITMASK\_CNT\_U32 | 1 | Counts | ((uint32)(0xFFFF0000U)) |
| LOWR16BITMASK\_CNT\_U32 | 1 | Counts | ((uint32)(0x0000FFFFU)) |

# Software Component Implementation

## Sub-Module Functions

## Init: ExcpnHndlgInit1

## Design Rationale

*Non-RTE function because it needs to be called before the OS is started - so that floating point exceptions can be enabled before anything uses floating point*

## Module Outputs

*None*

## Init: ExcpnHndlgInit2

## Design Rationale

*RTE function to initialize all the NTCs to pass*

## Module Outputs

*None*

## Per: ExcpnHndlgPer1

## Design Rationale

*RTE Periodic function called every 2 ms to check for OS errors*

## Store Module Inputs to Local copies

*Refer MDD*

## (Processing of function)………

*Triggered on Timing Event every 2ms*

## Store Local copy of outputs into Module Outputs

*None*

## Server Runables

## ChkForStrtUpTest

## Design Rationale

*Refer FDD*

## (Processing of function)………

*Refer FDD*

## FeNmiClkMonr0RtLowrLimFlt

## Design Rationale

*Refer FDD*

## (Processing of function)………

*Refer FDD*

## FeNmiClkMonr0RtUpprLimFlt

## Design Rationale

*Refer FDD*

## (Processing of function)………

*Refer FDD*

## FeNmiClkMonr1RtLowrLimFlt

## Design Rationale

*Refer FDD*

## (Processing of function)………

*Refer FDD*

## FeNmiClkMonr1RtUpprLimFlt

## Design Rationale

*Refer FDD*

## (Processing of function)………

*Refer FDD*

## FeNmiClkMonr2RtLowrLimFlt

## Design Rationale

*Refer FDD*

## (Processing of function)………

*Refer FDD*

## FeNmiClkMonr2RtUpprLimFlt

## Design Rationale

*Refer FDD*

## (Processing of function)………

*Refer FDD*

## FeNmiClkMonr3RtLowrLimFlt

## Design Rationale

*Refer FDD*

## (Processing of function)………

*Refer FDD*

## FeNmiClkMonr3RtUpprLimFlt

## Design Rationale

*Refer FDD*

## (Processing of function)………

*Refer FDD*

## FeNmiDmaTrf

## Design Rationale

*Refer FDD*

## (Processing of function)………

*Refer FDD*

## FeNmiDmaRegAcsProtnErr

## Design Rationale

*Refer FDD*

## (Processing of function)………

*Refer FDD*

## FeNmiEcmMstChkrCmp

## Design Rationale

*Refer FDD*

## (Processing of function)………

*Refer FDD*

## FeNmiOperModErrFlsProgmModStrtd

## Design Rationale

*Refer FDD*

## (Processing of function)………

*Refer FDD*

## FeNmiOperModErrSngChipInactv

## Design Rationale

*Refer FDD*

## (Processing of function)………

*Refer FDD*

## FeNmiOperModErrTestModStrtd

## Design Rationale

*Refer FDD*

## (Processing of function)………

*Refer FDD*

## FeNmiPeg

## Design Rationale

*Refer FDD*

## (Processing of function)………

*Refer FDD*

## FeNmiWdg

## Design Rationale

*Refer FDD*

## (Processing of function)………

*Refer FDD*

## GetMcuDiagcIdnData

## Design Rationale

*Refer FDD*

## (Processing of function)………

*Refer FDD*

## ProcMpuExcpnErr

## Design Rationale

*Refer FDD*

## (Processing of function)………

*Refer FDD*

## ProcNonCritOsErr

## Design Rationale

*Refer FDD*

## (Processing of function)………

*Refer FDD*

## ProcPrmntOsErr

## Design Rationale

*Refer FDD*

## (Processing of function)………

*Refer FDD*

## ProcPrvlgdInstrExcpnErr

## Design Rationale

*Refer FDD*

## (Processing of function)………

*Refer FDD*

## ProcUkwnExcpnErr

## Design Rationale

*Refer FDD*

## (Processing of function)………

*Refer FDD*

## SetMcuDiagcIdnData

## Design Rationale

*Refer FDD*

## (Processing of function)………

*Refer FDD*

## Interrupt Functions

## AlgnErrIrq

## Design Rationale

*Refer FDD*

## (Processing of the ISR function)…..

*Refer FDD*

## FpuErrIrq

## Design Rationale

*Refer FDD*

## (Processing of the ISR function)…..

*Refer FDD*

## SysErrIrq

## Design Rationale

*Refer FDD*

## (Processing of the ISR function)…..

*Refer FDD*

## ResdOperIrq

## Design Rationale

*Refer FDD*

## (Processing of the ISR function)…..

*Refer FDD*

## Module Internal (Local) Functions

## ProcStrtUpOrSwRst

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Function Name** | ProcStrtUpOrSwRst | Type | Min | Max |
| **Arguments Passed** | None |  |  |  |
|  |  |  |  |  |
| **Return Value** | NA |  |  |  |

## Design Rationale

*Refer FDD*

## Processing

## ProcEcmRst

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Function Name** | ProcEcmRst | Type | Min | Max |
| **Arguments Passed** | None |  |  |  |
|  |  |  |  |  |
| **Return Value** | NA |  |  |  |

## Design Rationale

*Refer FDD*

## Processing

## ProcPinRst

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Function Name** | ProcPinRst | Type | Min | Max |
| **Arguments Passed** | None |  |  |  |
|  |  |  |  |  |
| **Return Value** | NA |  |  |  |

## Design Rationale

*Refer FDD*

## Processing

## GLOBAL Function/Macro Definitions

<If these are numerous and defined in a separate source file then reference the source file only.>

## GLOBAL Function #1

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Function Name** | (Exact name used) | Type | Min | Max |
| **Arguments Passed** | (if none, write None) | <Refer MDD guidelines[1]> | <Refer MDD guidelines[1]> | <Refer MDD guidelines[1]> |
|  | (Insert more rows for additional passed arguments) |  |  |  |
| **Return Value** | (if no value returned, write N/A) |  |  |  |

## Design Rationale

## processing

(Place flowchart/design for local function)

# Known Limitations with Design

None

# UNIT TEST CONSIDERATION

None

Abbreviations and Acronyms

| **Abbreviation or Acronym** | **Description** |
| --- | --- |
|  |  |
|  |  |

Glossary

**Note**: Terms and definitions from the source “Nexteer Automotive” take precedence over all other definitions of the same term. Terms and definitions from the source “Nexteer Automotive” are formulated from multiple sources, including the following:

* ISO 9000
* ISO/IEC 12207
* ISO/IEC 15504
* Automotive SPICE® Process Reference Model (PRM)
* Automotive SPICE® Process Assessment Model (PAM)
* ISO/IEC 15288
* ISO 26262
* IEEE Standards
* SWEBOK
* PMBOK
* Existing Nexteer Automotive documentation

| **Term** | **Definition** | **Source** |
| --- | --- | --- |
| MDD | Module Design Document |  |
| DFD | Data Flow Diagram |  |

References

| **Ref. #** | **Title** | **Version** |
| --- | --- | --- |
| 1 | AUTOSAR Specification of Memory Mapping (Link:[AUTOSAR\_SWS\_MemoryMapping.pdf](http://www.autosar.org/download/R4.0/AUTOSAR_SWS_MemoryMapping.pdf)) | v1.3.0 R4.0 Rev 2 |
| 2 | MDD Guideline | EA4 01.00.01 |
| 3 | [Software Naming Conventions.doc](http://misagweb01.nexteer.com/eRoomReq/Files/erooms8/NextGeneration/0_fc55f/Software%20Naming%20Conventions%2003x(In%20Work).doc) | 1.0 |
| 4 | [Software Design and Coding Standards.doc](http://eroom1.nexteer.com/eRoomReq/Files/erooms8/NextGeneration/0_1a67a9/Software%20Design%20and%20Coding%20Standards.doc) | 2.1 |